The robot uses odometry in order to track its own location in a global frame. Using the simulated area created in the RViz program the robot determines in location